Distributed Multi-Robot Task Allocation through Vacancy Chains

Torbjørn S. Dahl Norwegian Defence Research Establishment (FFI) Postboks 25, 2027 Kjeller, Norway

Torbjorn-Semb.Dahl@ffi.no

Maja J. Matarić and Gaurav S. Sukhatme Center for Robotics and Embedded Systems University of Southern California 941 West 37th Place, Los Angeles, California 90089-0781

mataric|gaurav@usc.edu

Abstract

Existing multi-robot task allocation algorithms (MRTA) generally do not consider the effects of interaction, such as interference, but instead assume that tasks are independent. That assumption, however, is often violated in groups of cooperative mobile robots, where interaction effects can have a critical impact on performance. Modeling the effects of interaction, or group dynamics, is problematic due to their complexity and volatility, which also makes it difficult to hand-code optimal solutions to MRTA problems. We present a distributed MRTA algorithm that is sensitive to interaction dynamics. The algorithm uses distributed reinforcement learning to make interference-sensitive estimates of task utilities and relies on stigmergy to let optimal allocations emerge. The algorithm is inspired by vacancy chains, a resource distribution process common in human and animal societies. We present a formal model of task allocation through vacancy chains that defines optimal allocations in MRTA problems in terms of interference-sensitive measures of individual robot contributions. We validate our model by demonstrating, in simulation, how the predicted allocations are produced by our algorithm. As the robots continuously update their individual utility estimates, the vacancy chain algorithm has the additional property of adapting automatically to changes in the environment, e.g., robot breakdowns or changes in task values. We study the problem of cooperative transportation and demonstrate that our algorithm improves on the performance of hand-coded solutions. Finally, as the vacancy chain algorithm uses no communication or unique roles and is more robust and scalable than alternative algorithms with significant communication overheads.

1 Introduction

Existing multi-robot task allocation (MRTA) algorithms, generally assume task independence, i.e., they do not consider explicitly synergistic or interferencerelated effects on performance. Task independence is an important assumption in that it facilitates optimal task allocation, and in some problem domains it is reasonable to make. In cooperative mobile robotics however, it is generally not valid to assume that tasks are independent. In such systems, the effects of the interaction between robots working on different tasks, i.e., the group dynamics, commonly have a critical impact on performance.

Using scheduling [7] as a formalism for MRTA, we show that, in domains where the group dynamics have a significant effect on performance, this problem is N P-hard. This implies that finding optimal solutions using general algorithms is infeasible and that we instead need to look for helpful heuristics and practical ways of restricting the problem. The complexity of a group’s dynamics also makes it difficult to model the effects of these dynamics efficiently and accurately. It is possible to circumvent the modeling problem by estimating the task utilities under different allocations without an explicit model of the underlying dynamics. However, estimating the task utilities for all possible allocations can only be done when the number of robots and tasks is small, as the related number of possible allocations grows exponentially. Here we present a model of distributed MRTA as task allocation through vacancy chains (TAVC). The model explicitly handles the effects of the group dynamics and breaks down the system performance into individual robot contributions. This allows us to use the model as a basis for a distributed, communication free, MRTA algorithm that handles the complexity of this problem by using task utility estimates local to each robot and relying on stigmergy to let optimal solutions emerge. The effects of the group dynamics impact the local task utility estimates in a way that leads to the reliable emergence of allocations that are optimal according to the TAVC model. We demonstrate that the vacancy chain algorithm can improve the performance of a group of robots on a cooperative prioritized transportation problem beyond what is possible with hand-coded solutions.

2 Multi-Robot Task Allocation

MRTA is concerned with allocating tasks to robots. Gerkey and Matarić [13, 12] have presented a taxonomy of this domain over three dimensions: single-task robots vs. multi-task robots, single-robot tasks vs. multi-robot tasks, and instantaneous assignment vs. time-extended assignment. They also discuss several formalisms for expressing multi-robot task allocation problems. Here we explore further the scheduling formalism for MRTA in order to clarify the role of group dynamics and to demonstrate the complexity inherent in problems where their effects are significant. When MRTA is formalized as scheduling, the terms job and task, and the terms machine and robot, become interchangeable. We will use the terms job and machine when we relate the MRTA problem to other scheduling problems and the terms task and robot when we discuss the specifics of MRTA.

2.1 Problem Complexity

In an idealized form, MRTA is the problem of optimizing the allocation of tasks to robots over time, with respect to some given criteria. This problem can be formalized within the existing framework of scheduling [7]. Scheduling is a well studied problem domain and the complexity of many scheduling problems has been established. These results suggest what classes of algorithms may be applicable to different scheduling problems. Defining MRTA problems in terms of a scheduling formalism indicates what classes of algorithms are suitable for that problem.

Scheduling problems are described in terms of a set of machines M_j (j = 1, ..., m) that process a set of jobs J_i(i = 1, ..., n). Jobs may consist of a set of operations, O_{i1}, ..., O_{i,ni} . If any job can run on any machine, the machines are called parallel. Parallel machines are the most general instance of a class called multi-purpose machines (MP M). In MPM, a job can be processed on any machine which has the appropriate tools. If the machines in M_j are used simultaneously the scheduling problem is called a multiprocessor task scheduling problem. In the simplest case where n_i = 1, each job J_i has a related processing requirement p_i and a cost function f_i(t) reflecting the cost of completing J_i at time t. The cost function f_i may use a due date d_i and a weight w_i. Further constraints on precedence, preemptability, and batching of jobs are also common. The machine environment is also subject to a number of further formalizations. Parallel machines, for example, are divided into three classes: identical machines, P, uniform machines, Q, and unrelated machines, R. For identical machines, P, the processing time of a job J_i is the same on all machines M_j , i.e., p_{ij} = p_i. For uniform machines, Q each machine has a related speed s_j and the processing time of a job is dependent on the machine, i.e., p_{ij} = p_i/s_j . Lastly, for unrelated machines, R, the processing time may be dependent on the machine-job combination, i.e., p_{ij} = p_i/s_{ij} .

A common optimization criterion in scheduling is the weighted total flow time, denoted ∑ w_iC_i, where C_i is the finishing time of each job, J_i. Other common optimization criteria are defined with respect to other values than the total flow time, e.g., job earliness, job tardiness, or deviation from deadline. Scheduling problems in general can be denoted by three main features: the class of machines, the attributes of the jobs, and the function to be optimized, e.g., Q | p_i = p | ∑ f_i, denotes a problem with uniform machines and uniform task processing times, where the value to optimize is the sum of the cost. Some scheduling problems are solvable in polynomial time. Other scheduling problems, such as finding the minimal weighted total flow time for identical machines, P ‖ ∑ w_iC_i, have been shown to be N P-hard [7].

Formalizing the Effects of Robot Interaction For a given static environment, a group’s dynamics depend, to a large degree, on what machines the different jobs are allocated to, i.e., the allocation. We formally define an allocation to be a function from machines to jobs. For m machines and n jobs, this function can be represented as a vector A of size m, where vector element i indicates what job is allocated to machine i. We use ∅ to indicate a machine that has not been allocated a job. Intuitively, an allocation can be seen as a slice of a schedule as represented by a Gantt chart [7]. Figure 1 illustrates this for two allocations A_1 and A_2. The allocations are indicated by the dashed lines through a job-oriented schedule presented as a Gantt chart. The corresponding allocations are presented in Equations 1 and 2.

Figure 1: Job-Oriented Gantt chart

A_1 = [M1, M2, M3, ∅] (1)

A_2 = [∅, ∅, ∅, M1] (2)

MRTA with Interaction is N P-hard We suggest that the effects of group dynamics on job processing times i can be included in the formal scheduling framework by making the job processing time, p_i, from the time the job is started, t_s, to the time the job is finished, t_f , a function of the allocations during this time, A_{ts,tf} , as shown in Equation 3.

p_i = g_i(A_{ts,tf} ) (3)

We call the function g the interaction function. We call the class of machines whose performance is significantly affected by group dynamics interaction-dependent machines and denote the class using the subscript_{ID}. The interaction function, as a formalization of group dynamics, captures much of the complexity of group dynamics in otherwise static environments such as transportation between stationary locations. It is worth mentioning that this is not a suitable formalization of group dynamics in more dynamic problems, e.g., problems where the processing times are also dependent on a changing spatial distribution of jobs. An example of such a problem is cooperative tracking and pursuit [19].

Theorem 1 R_{ID} ‖ ∑ w_iC_i ∈ N P-hard

Proof 1 The optimization problem R ‖ ∑ w_iC_i describes a set of unrelated machines, R, a set of non-preemptable jobs, J_i, with related weights, w_i, and processing times, p_i. The machine speeds, s_{ij} , are job dependent. Unrelated machines are a sub-class of interaction-dependent machines in that the function describing the task processing time, p_{ij} = p_i/s_{ij} , is a deformed interaction function that is only dependent on the task and machine in question and not on what tasks are allocated to the other machines. We can create, in polynomial time, a corresponding problem R_{ID} ‖ ∑ w_iC_i with an identical set of machines, R_{ID}, an identical set of weighted jobs, but with task processing times described by the interaction function g_i(A_{ts,tf} ).

The assumption that the machines in the original problem are unrelated, but not interaction-dependent, implies that the value of g_i(A_{ts,tf} ) is only dependent on which machine M_j , the related job, J_i, is allocated to in the relevant allocations A_{ts,tf} . For non-preemptable jobs, M_j will be the same for all those allocations. The interaction functions g_i(A_{ts,tf} ) can be produced in polynomial time, by finding which machine job, J_i, is allocated to in the initial allocation, A_{ts} . The job, J_i, and machine M_j , can then be used to find the machine speed using the given function, p_i/s_{ij} .

An algorithm solving R ‖ ∑ w_iC_i problems uses sets of machines, sets of jobs, and optimization criteria that are identical to the ones used by an algorithm for solving the corresponding S ‖ ∑ w_iC_i problems. The only difference between the problems is the representation of the function for job processing times. We have shown how the function p_i/s_{ij} can be accurately represented in the more general form g_i(A_{ts,tf} ), and that the transformation can be done in polynomial time. Hence, an optimal solution to the new problem would be an optimal solution to the original problem. This again shows that R ‖ ∑ w_iC_i, which is N P − hard, reduces to R_{ID} ‖ ∑ w_iC_i which, ipso facto, must also be N P-hard. �

Spatially Classifiable Jobs As a way of reducing the complexity of the interaction function, the work presented here focuses initially on a particular class of problems where the jobs are spatially classifiable. Such jobs can be divided into a set of classes, K_k, where the interactions between machines working on tasks in different classes have no significant effects on the groups performance. In terms of scheduling, we denote spatially classifiable jobs sc. The problem of optimizing the weighted total flow time in a system with interaction-dependent machines and spatially classifiable jobs is denoted R_{ID} | sc | ∑ w_iC_i. One example of such problems is when classes of jobs take place in spatially separate areas. For such jobs, J_i, the processing time is a function of the effects of the interaction between the machines currently allocated to jobs in that class, A_{ts,tf ,k}, as expressed in Equation 4.

p_i = g_i(A_{ts,tf ,k}) (4)

The allocation of robots between jobs of other classes is not relevant. By the same reasoning as with general interaction-dependent jobs, it can be shown that scheduling spatially classifiable jobs over interaction-dependent machines is an N P-hard problem.

Homogeneous Robots Within the class of interaction-dependent machines processing spatially classifiable jobs, we restrict ourselves further to looking at problems where the machines are identical or homogeneous. In this case, the interaction function is dependent only on the number of robots, m_k, currently working on jobs in each class, K_k. The job processing time for this class is given in Equation 5.

p_i = g_i(m_k) (5)

The problem of scheduling with two or more identical machines, P 2 ‖ ∑ w_iC_i, is known to be N P-hard [7]. In this problem, the job processing time, p_i, is only dependent on the job, J_i. By the same reasoning as with unrelated interaction-dependent machines, it can be shown that P 2 ‖ ∑ w_iC_i reduces to P_{ID}2 ‖ ∑ w_iC_i, i.e., scheduling spatially classifiable jobs over two or more identical interaction-dependent machines. Hence, P_{ID}2 ‖ ∑ w_iC_i is also N P-hard.

2.2 Modeling Group Dynamics

The interaction function we defined in Section 2.1 describes the effects of all possible allocations on individual job processing times. Such a description presupposes that we can model these effects in a way that lets us identify the relevant times. This presumption, however, is too optimistic. In this section we review previous work on modeling the effects of interaction.

In groups of mobile robots, we term the internal interactions between members of the group the group dynamics. The group dynamics can help explain group-level behavioral features created by the presence of multiple robots, e.g., interference, when the robots have to spend time avoiding each other rather than following the paths that would be optimal in single-robot systems. The presence of multiple robots very commonly has a negative effect on performance in terms of interference. Cooperation, on the other hand, produces group dynamics that have a positive effect on performance. When group dynamics have a major effect of performance, understanding and modeling these dynamics is necessary in order to predict the value of different schedules. In embodied systems such as mobile robots, there is significant uncertainty related to interaction with the real world in terms of accuracy of perception and effects of actions. A model of the dynamics within a group of mobile robots is a model of several interacting systems, each with a significant level of inherent unpredictability. This limits the possible accuracy of any formal model.

Models of group dynamics have been divided into microscopic, which may or may not be simulation-based, and macroscopic [20]. Microscopic models explicitly represent each agent. Simulation-based models simulate the actions taken by each of the agents so that properties of the system can be recorded as the agents interact. Macroscopic models directly describe properties to systems on the basis of abstract features such as the number and general distribution of agents. Below we review the most relevant work on producing and using explicit models of group dynamics to improve group performance.

Microscopic Models Game theory [24] is an abstract model of multiple interacting agents as players in formalized n-person stochastic games. Game theory traditionally represents each player in terms of his/her strategy for playing a given game and its related payoff matrix for the possible moves. On the basis of these factors, game theory describes some of the resulting features of the ensuing games, e.g., their optimality and stability. A game theoretic approach to modeling group dynamics requires that we know the relevant payoff matrices. Unfortunately, this information is not known in most non-trivial multirobot systems. To overcome unknown payoff matrices, Littman [21] presented the Minimax-Q algorithm which is guaranteed to find the equilibrium of any stochastic game. As a general payoff policy for n tasks and m robots is of size n^m, it is not feasible in general to estimate the payoffs for each state/action combination. Bowling et al. [5] presented experimental data demonstrating how a reinforcement learning (RL) algorithm based on policy gradient ascent and the WoLF (Win or Learn Fast) principle for adjusting the learning rate can overcome this complexity. We discuss our approach to MRTA in terms of game theory in more detail in Section 8.

Simulation-Based Models Goldberg and Matarić [15] developed Augmented Markov Models, transition probability matrices with additional temporal information, to learn statistical models of interaction in a space of abstract behaviors. They also used these models to maximize reward in a multi-robot mine collection task.

Balch et al. [2] studied live insect colonies and constructed three-dimensional histograms of insect presence over a discretized area. The work was a step toward a long term goal of combining spatio-temporal models with Behavior Hidden Markov Models for behavior recognition [17] in order to recognize colony behaviors.

Yan and Matarić [31] have attempted multi-level modeling of group behaviors from spatial data describing both human and robot activity. Like Balch et al., they used three-dimensional histograms to recognize and describe different activity distributions as produced by underlying behaviors.

Seth [27] pointed out the distinction in biology between ‘phenomenological’ and ‘mechanistic’ models of interference, where the former identifies mathematical relationships between intake rates and agent density in empirical data while the latter constructs individual-based models with pre-specified rules for agent behavior. This distinction corresponds closely to that between macroscopic and simulation-based models used in robotics. Mechanistic models allow a derivation of the interaction between agent density and rule application with respect to intake rates. The phenomenological models assume that agents always optimize their individual intake rates. They also assume unstructured environments. These assumptions are often invalid both in biological systems and in the multi-robot task allocation domain. As an alternative to the traditional biological models, Seth presents a simulation-based model using genetic algorithms to evolve foraging behaviors for multiple agents in spatially explicit environments. The evolved systems are able to reproduce interference functions previously described in field studies of insects, but not reproduced by phenomenological models.

Macroscopic Models Matarić [22] proposed a macroscopic model of interference as an estimate based on group density. Group density is defined as the ratio between the agents’ footprints and the available interaction space. An agent’s footprint is its sphere of influence, including factors such as geometry, motion constraints, and sensor range. If only the number and size of the agents are used, a mean free path can be computed and used to estimate the number of expected collisions for agents executing random walks.

Lerman et al. [20] have studied three different types of models of cooperation and interference in groups of robots: sensor-based simulations, microscopic numerical models, and macroscopic numerical models. They used differential equations to model the group dynamics on a macroscopic level and showed that the three different models produced corresponding results. Unlike the sensorbased simulation and the microscopic numerical model, the macroscopic model had the advantage of being very fast and independent of the number of robots modeled. To make a macroscopic model tractable, however, many simplifying assumptions were necessary.

Macroscopic or phenomenological models are not generally sophisticated enough for optimizing specific task allocation algorithms. In particular, Matarić’s model for estimating interference does not consider synergistic effects or environmental complexity. The differential equation models produced by Lerman et al. similarly assume uniform distributions of robots and tasks. The simulation-based models or mechanistic models produce problem-specific solutions, but the time needed to construct those reners them unsuitable for use in MRTA algorithms. Currently there are no models of the effects of group dynamics with the speed, generality, and predictive accuracy necessary for specifying the effects of interaction on task processing times in MRTA problems with the aim of constructing optimal schedules. Simulation-based models are in general too slow while macroscopic mathematical models make too many simplifying assumptions to be of predictive use.

3 Task Allocation through Vacancy Chains

Corkill and Lesser [9] demonstrated that in the domain of coordination of distributed problem solving networks, the computational and communication cost of finding an optimal solution could outweigh the benefits such a solution brought over solutions produced using heuristic methods.

To deal with the two main problems of MRTA discussed above in Sections 2.1 and 2.2, we have developed the TAVC model of distributed MRTA. This model provides some heuristics for distributed MRTA. We used these to develop the TAVC algorithm, which produces optimal allocations as defined by the TAVC model. In Section 6 we present experimental results showing that the TAVC algorithm produces allocations that conform to the TAVC model and that it improves the performance of hand-coded solutions. In Section 8 we discuss the limitations of the TAVC model of MRTA with respect to more general models.

3.1 Vacancy Chains

The inspiration for our adaptive task allocation algorithm is the vacancy chain process [8], through which resources are distributed to consumers. The typical example is a bureaucracy where the retirement of a senior employee creates a vacancy that is filled by a less senior employee. This promotion, in turn, creates a second vacancy to be filled, and so on. The vacancies form a chain linked by the promotions. The resources distributed in this example are the positions and the consumers are the employees.

The general process of distributing resources in this way has been recognized in many different domains. It was originally reported in human populations relating to houses and apartments as well as to jobs in bureaucracies. Chase [8] proposed that major human consumer good such as cars, boats, and airplanes, also move through vacancy chains and that vacancy chains are common in other species such as the hermit crab, the octopus and different species of birds. In the case of the hermit crab, the empty gastropod shells they carry around as portable shelters are distributed through vacancy chains.

Chase lists three requirements for resource distribution through vacancy chains:

1. The resource must be reusable, discrete, and used by only one individual.

2. A vacancy is required before an individual takes a new resource unit, and individuals must need or desire new units periodically.

3. Vacant resource units must be scarce, and many individuals must occupy suboptimal units.

The vacancy chain resource distribution mechanism is both simple and powerful. It is based on stigmergy, unintentional communication between the consumers through their effects on the environment [18]. This makes distribution through vacancy chains robust and efficient in large groups/societies.

While distribution through vacancy chains ensures that the most attractive resources are consumed, it does not, like more sophisticated resource distribution mechanisms, take into account the quality of the consumer. As such, the vacancy chain distribution process can not exploit the possible advantages of distributing particular resources to particular consumers. The vacancy chain distribution mechanism treats all consumers as equals. In terms of task allocation, the vacancy chain distribution algorithm does not guarantee optimal allocations as it does not consider possible differences in machine speed. Our study of vacancy chain distribution reflects this fact by considering groups of homogeneous robots.

3.2 The Vacancy Chain Model of Distributed MRTA

Inspired by the vacancy chain process we developed a formal model describing how the allocation of tasks to machines influences system performance for spatially classifiable tasks. According to the TAVC model, any number of robots can be assigned to tasks from a given class. When a j’th robot is assigned to a task from a class, i, we say that service-slot (i, j) is filled.

A particular number of homogeneous robots, j, servicing the same class of tasks, i, will have a task processing frequency, c_{i,j} , dependent on the degree to which the robots are able to work concurrently without interfering with each other. The difference in task processing frequency, together with the task value, w_i, define the contribution of the last robot added, or the last service-slot filled, to the total system performance. We call this contribution, which can be negative, the slot-value, s_{i,j} . The formal definition is given in Equation 6.

s_{i,j} = w_i(c_{i,j} − c_{i,j−1}) (6)

When assigning an additional robot to a task leads to a decrease in the task processing frequency, the slot-value correspondingly becomes negative. When all the available service-slots have negative values, we say the task is saturated. If all the tasks are saturated, the system is saturated.

According to the TAVC model, an allocation is optimal when it maximizes the sum of the filled service slots. When the slot values decrease monotonically, optimizing the group performance becomes identical to optimizing the value of the individual slots. With spatially classifiable tasks and given the relevant slot-values, a group of robots can optimize the value of completed tasks over time, i.e., the throughput, by allocating robots to tasks or service-slots in order of decreasing slot-value. Note that this problem does not have the greedy-choice property as slot-value does not correspond to task-value and system performance is not necessarily optimized by allocating tasks from the class with the highest related value to all the robots. The total system performance or throughput value, T , for n robots, is simply the sum of the individual contributions as stated in Equation 7.

T_n = ∑ i ∑ j s_{i,j} (7)

In these kinds of problems, the task allocation algorithm can be distributed by letting each robot optimize the value of the service-slot it occupies.

In a scenario where the service-slots are allocated optimally, a failure in a robot will result in an empty service-slot. If the value of the vacant slot is greater than the value of one of the other occupied service-slots, the vacant slot will have to be filled in order to restore optimal allocation. Expressed in vacancy chain terminology, a vacant service-slot is a resource to be distributed between the robots.

3.3 The TAVC Algorithm

RL provides a way to improve on hand-coded solutions. Such improvements are particularly effective for problems where it is hard for human programmers to identify optimal solutions. One such problem is MRTA, where, as discussed in Section 2.2, the group dynamics make it difficult to identify optimal allocations. We have previously studied the use of distributed RL as a way of optimizing the performance of multi-robot systems in an interaction-sensitive manner [10]. Our TAVC algorithm is a specialization of that work for MRTA. In the TAVC algorithm, an action, as known from the RL literature, corresponds to a task, as known from the MRTA literature. Each robot keeps local estimates of task utilities in form of Q-values, and choose its tasks using an ϵ-greedy action selection function.

Q-learning is not sensitive to the frequency of rewards. Hence, the estimated values of actions do not necessarily correspond to their contribution to performance over time. In order to use Q-learning to optimize performance over time, it is necessary to make the temporal aspect of performance explicit in the reward function. Such a reward function, using the last task processing time, t, and task value, w_i, is given in Equation 8.

r = w_i/t (8)

This reward function promotes the actions with the highest contributions to the system performance because these will on average provide a higher reward. If a robot consistently occupies a service-slot that is suboptimal due to too much interference, the increased average traversal time will reduce the average reward for that slot below the average reward of the optimal service-slots. This change in average reward will attract the robot back to an optimal slot. Equation 9 clarifies the relationship between the definitions above by expressing the relationship between the individual throughput, T_i, the weighted differences in task completion frequencies, the weighted average task processing times and the average rewards, for j robots servicing a given task, i.

T_i = ∑ j s_{i,j} = w_i ∑ j (c_{i,j} − c_{i,j−1}) = w_i ∑ j 1 t_{i,j} = ∑ j r_{i,j} (9)

4 The Prioritized Transportation Problem

Cooperative transportation is a MRTA problem where group dynamics can have a critical impact on performance. It is also possible to construct spatially classifiable instances of this problem, which allows us to reduce the complexity of the group dynamics. This reduced complexity facilitates the initial study of algorithms for dealing with group dynamics in MRTA.

In the basic transportation problem, a group of robots traverse a given environment in order to transport items between the sources and the sinks. We call the time taken to traverse the environment once from a sink via a source and back to a sink the traversal time. To perform optimally on this task the robots must maximize the number of traversals in general. The basic transportation problem [10] is one of the sub-problems of foraging [1, 16, 25]. If the locations of sources and sinks are given, the foraging problem is reduced to a problem of transportation. Here we present the prioritized transportation problem, which generalizes the basic transportation problem to problems where the sources and sinks are divided into sets of different priority. Cooperative transportation is a general MRTA problem and the work presented here on prioritized transportation therefore provides important insights into the behavior of practical multi-robot systems in general.

When there is a source close to each sink and sinks are far apart, the optimal allocation is to have robots distributed over the local source/sink pairs or circuits, so as to avoid the increased traversal time implied by crossing between circuits. To optimize its performance on the prioritized transportation problem, a group of robots must strike the correct balance between different target values and different traversal times, as defined by the amount of interference on each circuit. We consider fetching and delivering one puck to be one task. In terms of scheduling, each transportation task corresponds to a job and the traversal times correspond to job processing times. The value of a task/job corresponds to its weight. The robots correspond to machines and, since their allocation has a significant effect on the performance of the system, the robots/machines are interaction-dependent. When the sources and sinks are distributed so as to make the tasks/jobs spatially classifiable, the problem of optimizing throughput in prioritized transportation is an instance of either R_{ID} | sc | ∑ w_iC_i or P 2_{ID} | sc | ∑ w_iC_i, according to whether the robots are heterogeneous or homogeneous. In Section 2, we showed both of these problems to be N P-hard.

5 Experimental Design

The goal of our experiments was to show both that the allocations produced by the TAVC algorithm satisfied the predictions of the TAVC model and that the group’s performance improved on the performance of hand-coded solutions. To show this we designed three experiments:

1. Base Distribution: The goal of this experiment was to demonstrate that the TAVC algorithm distributed six robots over two tasks of different value in an optimal way according to the TAVC model.

2. Filling a Vacancy: This experiment was designed to demonstrate that the TAVC algorithm could recover from a change in the optimal allocation by filling a vacancy. We created a vacancy by removing one of the robots occupying a high-value service slot. According to the TAVC model, this vacancy should be filled by one of the robots servicing a lowvalue service-slot in order to retain an optimal allocation. By retaining optimality, the TAVC algorithm would demonstrate that it can improve on the performance of hand-coded solutions. The TAVC algorithm is a general algorithm for retaining optimality, while hand-coded solutions must be specialized to each problem based on a model of the group dynamics. We argued in Section 2.2 that high-quality models of group dynamics are difficult to construct.

3. Breakdown without Vacancy: This experiment was a control experiment showing that, in accordance with the TAVC model, the removal of a robot servicing a low-value service slot did not lead to a change in the allocation of the remaining robots.

Together, these three experiments demonstrate that the TAVC algorithm establishes and maintains optimal allocations as defined by the TAVC model. To show that the performance improvement in our experiments are due to the TAVC algorithm, we also ran the three control experiments using robots that randomly chose between the available tasks. To show how the vacancy chain algorithm outperforms hand-coded MRTA algorithms, we ran an experiment where the assumed optimal allocations for the initial setup was hand-coded in the robot controllers. We emphasize that in general it is not possible to reliably identify this allocation and that this is the initial motivation for this work.

5.1 The Simulated Environment

The experiments were done in simulation on the popular Player robot device server and Stage simulater [14] software platform. From experience, controllers written for the Stage simulator work with little or no modification on real Pioneer mobile robots. The robots in the experiments were simulated Pioneer 2DX robots with SICK laser range-finders and PTZ color cameras. Each robot wore colored markings that could be recognized using ActiveMedia’s Color-Tracking Software (ACTS). The prototype markings as they appear on a real Pioneer 2DX are shown in Figure 2.

The experiments took place in a simulated twelve by eight meter environment with six robots and two sets of sources and sinks. Figure 3 shows a graphical rendering of the simulated environment in which the experiments took place, with the circuits indicated by dashed arrows and the sources and sinks labeled.

The sources and sinks were simulated laser bar-codes made from highly reflective material and recognizable by the laser range finder. We did not require actual objects to be carried. A proximity of less than 1 meter to a source or sink was interpreted as a delivery or a pick-up. The relatively high number of robots and a relatively low number of sources and sinks, or task classes, emphasizes the fact that the dominant factor in the complexity of multi-robot task allocation of spatially classifiable tasks is the number of robots, not the number of tasks.

Figure 2: Prototype Pioneer 2DX with Color Markings

Figure 3: The Simulated Environment with Circuits Indicated

5.2 Controller Architecture

All the robots in our demonstration used the same behavior-based controller [?]. However, our TAVC algorithm is independent of the underlying architecture, being defined purely in terms of distributed RL over problem states and task utilities. Based on individual experience our robots learned to specialize. However, they always retained a certain level of exploration that allowed them to find and fill new vacancies.

The State/Action Space Each controller in our experiments had a set of pre-programmed high-level behaviors. Each behavior corresponded to servicing one of the available tasks and consisted of multiple shared lower level behaviors. The low-level behaviors were as follows:

• obstacle avoidance: avoided obstacles detected (by laser range finder) in the desired path.

• visible target approach: approached the desired target when it was visible (to the laser range finder).

• target location approach: approached the location of the desired target when the target itself was not visible.

• wall following: followed the walls to the first available target when the desired target was not visible and localization (based on odometry) was deemed to be inaccurate.

The localization was deemed to be inaccurate whenever the desired target was not visible, but should have been so according to the robot’s estimated position and orientation. On encountering a target, the localization estimate was reset and again deemed to be accurate.

Individual Learning The robots were homogeneous with respect to hardware configuration and control algorithms. Each robot used RL to associate the currently observed problem state with the available actions, i.e., task-related behaviors. Over time, the RL differentiated the group by specializing robots on different tasks. The robots used temporal difference Q-learning [28] to associate the different states with one of the high-level task-related behaviors. The Qtables ware initialized with random values between −0.1 and 0.1, the learning rate α was set to 0.1, and the discount factor γ was set to 0.95.

The input- or state-space reflected which circuit the robot had used for its last traversal. This allowed the robots to learn policies that were not dedicated to one circuit. The learned policies could switch between circuits in order to construct optimal task sequences. In spite of this, the robots consistently learned a set of policies dedicated to a single circuit.

The action space corresponded to the available tasks. For action selection we used a greedy-ϵ strategy [28], where ϵ was set to 0.1. Because we wanted the system to remain adaptive to changes in the environment, we did not decrease ϵ over time, as is common.

5.3 Reward Function

In order to demonstrate the emergence of a vacancy chain structure, we designed a set of rewards that would promote the allocations predicted by the TAVC model. We call the circuit with the highest related reward the high-value circuit and, correspondingly, the circuit with the lowest related reward the low-value circuit. Specifically, in order to produce an initial allocation where three robots serviced one circuit and three robots serviced the other, it was necessary that it was less attractive to be one of four robots servicing the high-value circuit than to be one of three servicing the low-value circuit. This constraint on the reward function is presented formally in Equation 10.

∀(x, y).r_{x,4} < r_{y,3} (10)

In order for a vacancy in the high-value circuit to be filled, it must be more attractive to be the third robot in that circuit than to be the third robot in the low-value circuit. This is expressed formally in Equation 11, where p denotes the preferred circuit.

∀(x ≠ p).r_{x,3} < r_{p,3} (11)

We empirically estimated the relevant average traversal times. To satisfy the constraints given these times, we chose the circuit values in Equation 8 to be w_1 = 2200 and w_2 = 2000. We emphasize that the robots do not keep any information about the task values and that the optimal allocation emerges as each robot’s utility estimates converge as a result of individual experience only. The fact that the robots are oblivious to task values also allows new allocations to emerge when external factors such as the task values or the group size change.

6 Results

We performed the three main experiments defined in Section 5 as well as a number of supporting experiments. The resulting data are presented and analyzed below. Our student-t tests for statistical significance are all done with respect to a 90% confidence level. For each experiment we defined a convergence period and a stable period according to the stability of the system performance.

6.1 Base Distribution

This experiment used six robots. It consisted of 20 10-hour trials, each averaging 3000 traversals in total or 500 traversals per robot. The convergence period was 2.5 hours.

To evaluate performance, we consider the last target visited by each robot. This gives seven possible system states. We refer to each state using the notation h : l, where h is the number of robots whose last target was on the high-value circuit. Correspondingly, l is the number of robots whose last target was on the low-value circuit. The rows labeled T AV C in Table 1 show the mean, μ̂, and standard deviation, s, of the time the system spent in each of the states. The values are percentages of the total stable period. The rows labeled R describe the same values for a set of 20 trials using a group of robots that randomly chose between tasks.

State 0:6 1:5 2:4 3:3 4:2 5:1 6:1 TAVC μ̂ 0.1 2.7 19.0 41.8 29.3 6.6 0.5 s 0.3 1.9 7.7 6.6 9.0 3.2 0.5 R μ̂ 2.0 7.2 22.6 34.5 24.7 8.2 0.7 s 0.6 2.9 3.4 3.1 3.3 3.1 0.4 T 1.6 9.4 23.4 31.2 23.4 9.4 1.6

Table 1: State-Time Distributions for Six Robots

The row labeled T lists the number of different ways to choose a sample of size n from a population of m, as percentage of all possible samples, according to Equation 12. It is worth noticing that the time distribution produced by random allocation is closely aligned with this theoretical estimate, though the differences are statistically significant. T = m! n!(m − n!)2^m

(12)

The two time distributions given in Table 1 are presented as histograms in Figure 4 with the standard deviation indicated by the error bars for each state.

Figure 4: The State-Time Distributions of Six Randomly Allocated Robots and Six TAVC-Controlled Robots

Over 20 experiments, the difference in time spent in state 3 : 3 is statistically significant. The time the TAVC-controlled group spent in state 3 : 3 is also statistically higher than the time spent in any of the other states. This confirms that the group’s action-selection policies have converged to promote the state defined as optimal by the TAVC model, given the estimated task-processing times.

Figure 5 presents the average performance of a group of robots controlled by the vacancy chain algorithm over both the convergence period and the stable period. This group’s performance is indicated by the thick, solid line. The average performance of random allocation is indicated by the dashed line. The performance is calculated as the sum of the delivery frequencies for each circuit weighted by the value of the task.

Figure 5: The Performance of TAVC and Random Allocation for Six Robots

The performance data show that a group of robots controlled by the TAVC algorithm performs significantly higher than six randomly allocated robots. Together, the time distribution data and the performance data show that the adaptive controllers improve the group’s performance by adopting a dedicated service structure that conforms to the predictions of the TAVC model.

6.2 Filling a Vacancy

This experiment used five robots. We removed randomly one of the three robots that were servicing the high-value circuit at the end of the previous experiment, thus creating a vacancy on that circuit according to the TAVC model. The experiment consisted of 20 10-hour trials. The convergence period was 2.5 hours.

State 0:5 1:4 2:3 3:2 4:1 5:0 TAVC μ̂ 0.8 7.8 31.1 40.7 17.7 1.8 s 1.1 5.1 6.3 5.3 5.9 1.6 R μ̂ 2.6 12.6 32.4 34.8 15.5 2.1 s 0.9 2.2 4.0 2.3 3.7 0.4 C 3.1 15.6 31.3 31.3 15.6 3.1

Table 2: State-Time Distributions of Five Robots after a Breakdown Created a Vacancy on the High-Value Circuit

Figure 6: The State-Time Distributions of Five Randomly Allocated and Five TAVC-Controlled Robots After a Breakdown Created a Vacancy on the High- Value Circuit

The converged TAVC algorithm kept the system in state 3 : 2 for a significantly larger amount of time than a group of five randomly allocated robots. The time distributions are given in Table 2 and a graphical presentation if provided in Figure 6. This showed that the group had adapted its structure from one that promoted the 3 : 3 state to one that promoted the 3 : 2 state. The change demonstrated that a robot from the low-value circuit had filled the vacancy we had created in the high-value circuit.

The performance data presented in Figure 7 show that the removal of a robot from the high-value circuit caused the performance to drop sharply. After the re-convergence period, the performance rose again to a level that was significantly higher than the performance of random allocation and also significantly higher than the mean performance, over 20 trials, of a group of robots controlled by a hand-coded allocation algorithm optimized for six robots. The average performance of that group is indicated by the thin solid line.

Figure 7: The Performance of TAVC, Random Allocation and Hand-Coded Control before and after a Breakdown Creating a Vacancy on the High-Value Circuit

6.3 Breakdown without Vacancy

This experiments used five robots from the end of the first experiment. We removed randomly one robot from the low-value circuit. According to the TAVC model, this did not create a vacancy and, hence, the system was expected to remain in the 3 : 2 state. The experiment consisted of 20 10-hour trials, and the convergence time was 2.5 hours.

The state-time distribution during the stable period of this experiment, presented in Table 3, was not significantly different from the distribution produced during the second experiment presented in Section 6.2.

State 0:5 1:4 2:3 3:2 4:1 5:0 μ̂ 0.3 6.7 34.6 47.1 10.5 0.7 s 0.3 3.7 9.2 9.4 3.8 0.4

Table 3: State-Time Distributions after a Breakdown that did not create a Vacancy

As shown in Figure 8, performance fell significantly when the robot was removed, but remained significantly higher that the performance of five random controllers. There was no significant difference in the performance during the stable period of this experiment and the stable period of the second experiment where a vacancy was created. Also, there was no significant difference in performance between the convergence and stable periods of this, third, experiment. This consistency in the performance reflects the fact that the group structure remained unchanged.

Figure 8: The Performance of TAVC and Random Allocation before and after a Breakdown that did not create a Vacancy

The result demonstrates that the TAVC algorithm produces the allocations defined as optimal by the TAVC model, independently of which robot it is that breaks down.

7 Related Work

A number of algorithms for MRTA already exist. Below, in Section 7.1, we review a selection of the most prominent of these algorithms and discuss how their different approaches to group dynamics affect their applicability in domains where the effects these dynamics have a significant impact on group performance.

One way of dealing with N P-hard problems is to use heuristic algorithms that produce suboptimal but satisfactory solutions. Learning such heuristics in the domain of scheduling is a well-studied problem. Below, in Section 7.2, we present a selection of successful uses of machine learning (ML) as a way of finding heuristics for scheduling. We also discuss the applicability of these algorithms in domain of MRTA.

7.1 Previous Work on Multi-Robot Task Allocation

Botelho and Alami’s M+ algorithm [4] used a task allocation protocol based on the Contract Net protocol with formalized capabilities and task costs. The need to pre-define the capabilities and costs limits the applicability of the M+ algorithm to domains where these are known. It might, however, be possible to use the M+ algorithm with local utility estimates based on ML rather then hand-coded capabilities and costs. Gerkey and Matarić’s MURDOCH system [11], also based on the contract net protocol, used a set of metrics to locally score the suitability of the participating robots, a publish/subscribe protocol for communication, and an auction mechanism for task allocation. As with the M+ algorithm, the hand-coded suitability estimates have limited applicability, but the MURDOCH system can also use local task utility estimates based on ML. Werger and Matarić’s work on the Broadcast of Local Eligibility (BLE) algorithm for task allocation compares locally decided eligibilities to allocate tasks using Port Arbitrated Behaviors [30], an inter-robot coordination mechanism based on a fully connected communication network. Their example of Cooperative Multi-Robot Observation of Multiple Moving Targets used spatial proximity as a measure of eligibility, but BLE can also use eligibility estimates based on ML. In the L-ALLIANCE work by Parker [26], each robot explicitly estimates its own performance and the performance of other robots on selected tasks and uses these values to reallocate tasks by taking them over or acquiescing. The L-ALLIANCE algorithm uses local utility estimates to make local allocation decision, but needs pre-programmed estimation procedures that reduce the general applicability of this algorithm.

We are not aware of any existing general MRTA algorithms that explicitly handle the effects of group dynamics. As such, the TAVC algorithm represents an attractive alternative for domains where the effects of these dynamics have a significant impact on system performance.

7.2 Learning Approaches to Task Allocation

Zhang and Dietterich [32] presented a RL approach to scheduling that learned domain specific heuristics for the scheduling procedure. The state space consisted of possible schedules and actions were possible changes to the schedules. The system learned what changes would quickly create feasible schedules with maximized capacity utilization. The problem domain considered was space shuttle payload processing.

Zomaya et al. [33] presented another algorithm for learning scheduling heuristics. Their algorithm learned dynamic scheduling, i.e., scheduling when there is no a priori knowledge about the tasks. It used a back-propagation neural network and a history queue that functions like an eligibility trace to learn how to associate a set of job parameters with a set of machines.

Both above algorithm are general and applicable to all scheduling problems. However, they rely on a centralized learning mechanism, which can fail critically due to robot breakdown and also does not scale easily to large groups.

Brauer and Weiß [6] used the multi-agent learning paradigm to distribute the learning of heuristics for scheduling a set of multi-operation jobs over a set of machines. The operations were totally ordered and each operation could only be performed by a subsets of machines. Using RL, each machine estimated the efficiency of the possible predecessors and together the machines learned to improve the total production rate from an initial state where all machines were assumed to be equally efficient. Brauer and Weiß also showed that the learning allowed the system to adapt to machine breakdowns. This algorithm, however, is restricted to completely ordered jobs and this limits its applicability to general scheduling and task allocation problems.

Blum and Sampels [3] studied different pheromone representations in ant colony optimization of first order job shop scheduling. Each job traversed a set of machines by stochastically selecting machines in accordance with a given set of constraints on the job’s operations. Throughout the traversal, the system updated a pheromone trace, effectively learning environmentally embedded heuristics for scheduling. The different pheromone representations allowed the system to estimate utilities for different combinations of machines, including estimating the utility of a machine in isolation and the utility of a machine depending on the last machine visited. This algorithm, however, is limited to jobs that consist of multiple operations. It is difficult to see how a similar pheromone trail could be used successfully as a general scheduling algorithm.

Tangamchit et al. [29] used distributed RL on a set of robots to allocate patrolling tasks. Each robot locally estimated the utility of a set of patrolling points and together learned to divide the set of point between them in an optimal manner. Tangamchit et al. also used local and global proximity measures as heuristics for action selection in order to speed up learning. The specificity of the spatial heuristics limits the applicability of this algorithm to general task allocation problems.

The work reviewed above demonstrates the use of ML techniques to learn successful heuristics for scheduling. The heuristics can be centralized, environmentally embedded, or distributed. However, the domains considered in all of the work reviewed above, except for the work by Tangamchit et al., do not have significant effects from group dynamics. In spite of this, all the learning algorithms reviewed above would likely improve a group’s performance in the presence of significant effects from group dynamics, as they in general learn where to allocate jobs according to feedback based on processing time. The advantage of our vacancy chain algorithm over existing learning algorithms for scheduling is the combination of its general applicability and its distributed learning mechanism.

8 Discussion

Our experiments showed that the TAVC algorithm is an efficient and robust MRTA algorithm. The fact that the TAVC algorithm needs only a minimal amount of information about any particular problem domain makes it potentially applicable to a large class of problems. We demonstrated that in spite of the difficulties related to modeling group dynamics and the general complexity of scheduling, it is possible, under certain restrictions, to use the interference sensitive TAVC algorithm to improve on random allocation and on hand-coded solutions. It would have been informative to compare the performance of the TAVC algorithm to other known ML-based algorithms such as the progress estimation-based algorithm used by the L-ALLIANCE system [26] or a more general algorithm based on, e.g., Markov games [21]. Such algorithms may or may not outperform the TAVC algorithm. However, the fundamental difference between such solution and the TAVC algorithm is that the TAVC algorithm works without any explicit communication, while other algorithms imply communication overheads. For example, in L-ALLIANCE, each robot explicitly estimates the progress of other robots, and for Markov games, the global state has to be communicated in order to satisfy the Markov property.

Our work on the TAVC algorithm has brought up several issues that do not relate directly to the experimental results. Below we discuss the most important of those in some detail.

8.1 Applicability

The inspiration for the vacancy chain algorithm and the experimental results presented here are all taken from the multi-robot domain. As a general scheduling algorithm it is interesting to evaluate the applicability of the vacancy chain algorithm outside that domain. All domains where cooperation and/or competition provide significant effects from group dynamics are possible candidate problems for the vacancy chain algorithm. One example is network load minimization for distributed cooperating processes. In this domain, different distributions, or allocations, imply different communication loads. A group of migrating processes, using the TAVC algorithm, could, in this domain, converge on distributions that would minimize the network load.

In general, in order to optimize an allocation problem using the TAVC algorithm, the jobs must be spatially classifiable, i.e., the effects of interaction must be restricted to work within classes of jobs. Also, the machines must be able to choose between the jobs, and the quality of each job solved must also be available to each machine to provide feedback to the local utility estimates.

8.2 Optimality and Stability

A group of non-communicating, adaptive, greedy robots can be seen as participants in a multi-player game and as such, the group behavior can be analyzed using game theory [24]. To converge to a stable solution, the TAVC algorithm depends on finding allocations where no single robot can benefit from unilaterally changing tasks. In game theory, such allocations are called Nash equilibria. Another important result from game theory is that some problems have suboptimal Nash equilibria, and some problems do not have Nash equilibria, unless we consider mixed strategies. Mixed strategies are not practical as we have placed a limiting factor on switching between classes of tasks in our definition of spatially classifiable tasks in Section 2.1. Problems with suboptimal Nash equilibria, as discussed below, would lead to suboptimal allocations. On problems without Nash equilibria, the TAVC algorithm would not converge.

Optimality Consider two robots, m_1 and m_2, and two task classes, k_1 and k_2, with identical values. Assuming identical traversal times and identical start and finishing times, the interaction function defined in Equation 13 will lead to convergence on a suboptimal allocation.

g_i(A) =

3 if A = [k_1, k_1] 2 if only m_i serves k_1 5 if only m_i serves k_2 4 if A = [k_2, k_2]

(13)

This interaction function assumes that some allocations produce synergistic effects. One example of a synergistic effect is when the robots need to continuously repair a degrading path, e.g., by removing obstacles that appear on a regular basis. In this case, the average traversal time for two robots can be higher than for one robot.

The average processing time matrix corresponding to the interaction function presented in Equation 13 is presented in Table 4. This matrix shows the expected average processing time, g_1(A)/g_2(A) for m_1 and m_2 servicing task classes k_1 and k_2.

The optimal allocation, with the minimal processing times for the interaction functions given above, is [k_1, k_1], with the minimal total average processing time 4. The individual reward, due to the lower processing time, for a robot when unilaterally changing to task k_2 or defecting will likely be reflected in both the robots’ task utility estimates. With an exploration rate, ϵ, below 0.5, the majority of the exploratory changes will, on average, be unilateral. This is m_2 k_1 k_2 m_1 k_1 3/3 5/2 k_2 2/5 4/4

Table 4: Processing Time Matrix Leading to Sub-Optimal Allocation

likely to lead to one of the robots eventually changing tasks. In game theory, a problem with this structure is called a prisoner’s dilemma, and a unilateral change away from an optimal solution for individual gain is called a defection. The defection of one robot will increase the remaining robot’s processing time on k_1 task and eventually force it to defect as well. Intuitively, k_2 tasks will look more attractive due to the lower repair load, but turns out to be worse due to high levels of interference, e.g., due to less available space.

An exploration rate of less than 0.5 will inhibit the robots from returning to the [k_1, k_1] allocation, as most exploratory changes are unilaterally and will yield a reward lower than the one for the [k_2, k_2] allocation.

Instability It is possible, with heterogeneous robots, to construct processing time matrices that imply an ever-changing allocation. In game theory these are games without Nash equilibria. One such processing time matrix is given in Table 5.

m_2 k_1 k_2 m_1 k_1 2/2 4/1 k_2 4/1 2/2

Table 5: Unstable Processing Time Matrix

With the job processing time matrix presented in Table 5, there will always be an incentive for m_1 to change in order to be working alone on a task. For m_2, on the other hand, it will always be advantageous to change in order to work on the same task as m_1. This will leave the system in a constant state of change, not settling on any of the optimal allocations.

8.3 Allocation Strategies

The goal of MRTA is not necessarily to maximize throughput. Keeping general geographical patterns can be another possible goal. Theoretically the TAVC algorithm can be manipulated through the reward function to produce specific allocations. In dynamic environments and when robots are subject to individual failures, the adaptive properties can then be used to establish desirable allocations for varying numbers of active robots. Below we briefly discuss reward design for throughput- and pattern-based allocation.

Throughput-Based Allocation The reward functions we used in our experiments were designed to promote the desired 3 : 3 allocation given the estimated mean processing times. For given task values, the TAVC algorithm will produce allocations that optimized the throughput of the system. Optimizing the throughput value implies finding a balance between task value and robot interference. Equation 7 formalizes this implication for applications that satisfy the restrictions of the TAVC model.

Slot-Based Allocation Patterns As demonstrated by our first experiment, reward functions can also be used to produce pre-specified allocations. This type of MRTA can be desirable in problem domains such as patrolling [29].

The desired allocation for any number of working robots can be specified through slot-values. By providing task values that produce unique slot-values, we can have any allocation emerge. The TAVC algorithm will allocate tasks to robots according to the specified patterns by ensuring that the high-value service-slots are always filled.

Imagine an application where it is desirable to have at least two robots dedicated to a task A. However, if there are also two robots dedicated to task B, then it is preferable to have the fifth robot helping on task A rather than B. One imaginable scenario demanding this kind of configuration is the exploration and analysis of unknown environments. In this scenario it can be important to always have two robots dedicated to exploring the environment and localization of places of interest. If a place of interest is found and more robots are available, then two other robots should analyze the interesting site. If no further robots are necessary for the analysis, any other available robots should aid in the exploration.

A ranking, R, of the service-slots in such a scenario is a vector of serviceslots, as presented in Equation 14.

R = [(1, 1), (1, 2), (2, 1), (2, 2), (1, 3), (2, 3), (2, 4)] (14)

We assume that unlisted service-slots all have the same ranking, one higher than the number of listed service-slots. This allocation is presented graphically in Figure 9.

Figure 9: Service Slot Ranking for Slot-Based Allocation

The purpose of the reward function is to reflect the desired allocation and, as a result, the values it produces must satisfy the constraints the allocation imposes. This assumes a model of the effects of the group dynamics, something we argued in Section 2.2 was difficult to construct. Depending on the desired level of control, a less complete model could be satisfactory. We have demonstrated how this can be done by producing a desired allocation in our first experiment. For this experiment, the mean task processing time showed itself to be a reliable indicator of the number of robots currently servicing the task, and hence the number of slots currently filled.

If the interaction function is not injective, but one-to-many, different or additional indicators must be used to allow the state estimator to differentiate between states with identical task processing times.

8.4 Commitment vs Opportunism

Østergaard, Matarić, and Sukhatme [23] have empirically studied the role of commitment and opportunism in task allocation, defining a parameter space over which different degrees of these are preferable. The exploration rate, ϵ, and learning rate, α, together with the reward function, decide how easily our robots switch between tasks. By adjusting these parameters, a wide spectrum of commitment levels is available.

9 Future Work

Most other multi-robot task allocation algorithms, like MURDOCH [11], L- ALLIANCE [26], BLE [30], and M+ [4], can allocate tasks efficiently also for heterogeneous robots with different individual performance levels. We intend to conduct experiments with a modified vacancy chain task allocation algorithm using a static, non-Boltzmann softmax action selection function rather than the ϵ-greedy function we used in the experiments presented here. A softmax action selection function might allow the vacancy chain algorithm to solve the problem of allocating tasks among heterogeneous robots. A softmax function relates difference in utility to probability of selection. This indicates that high performing robots should have a higher probability of establishing themselves in the high-value service-slots. Since the vacancy chain algorithm is completely distributed, needs only a minimal amount of information about the problem at hand, and does not use any communication, it will be an attractive alternative to existing task allocation algorithms for domains with complex or unfamiliar dynamics.

The prioritized transportation problem has a very restricted interaction function which reduces the scheduling complexity. In the future we would also like to explore problems with more complex interaction functions in order to see how generally applicable the vacancy chain algorithm is.

Vacancy chain distribution only partially describes the distribution mechanism used to distribute shells among hermit crabs. It is also common for crabs to fight over shells [8]. Inspired by such negotiated resource exchanges it might be possible to produce algorithms that go further in allocating high resources to high quality consumers. We intend to study local interactions in an attempt to generalize the vacancy chain task allocation algorithm to groups of heterogeneous robots.

Acknowledgments

This work was supported in part by the Department of Energy (DOE) Robotics and Intelligent Machines (RIM) Grant DE-FG03-01ER45905 and in part by the Office of Naval Research (ONR) Defense University Research Instrumentation Program (DURIP) Grant 00014-00-1-0638.

References

[1] Tucker R. Balch. The impact of diversity on performance in multi-robot foraging. In Oren Etzioni, Jörg P. Müller, and Jeffrey M. Bradshaw, editors, The proceedings of the Third International Conference on Autonomous Agents (Agents’99), pages 92–99, Seattle, Washington, May 1 - 5 1999. ACM Press.

[2] Tucker R. Balch, Zia Khan, and Manuela M. Veloso. Automatically tracking and analyzing the behavior of live insect colonies. In Jörg P. Müller, Elisabeth Andre, Sandip Sen, and Claude Frasson, editors, Proceedings of the Fifth International Conference on Autonomous Agents (Agents’01), pages 521–528, Montreal, Canada, May 31 - June 4 2001. ACM Press.

[3] Christian Blum and Michael Sampels. Ant colony optimization for fop shop scheduling: A case study on different pheromone representations. In Proceedings of the 2002 Congress on Evolutionary Computing (CEC’02), pages 1558–1563, Honolulu, Hawaii, May 12 - 17 2002. IEEE Press.

[4] Silvia Botelho and Rachid Alami. M+ : a scheme for multi-robot cooperation through negotiated task allocation and achievemen. In Proceedings of the 1999 IEEE International Conference on Robotics and Automation (ICRA’99), pages 1234–1239, Detroit, Michigan, May 10-15 1999. IEEE Press.

[5] Michael Bowling and Manuela M. Veloso. Rational and convergent learning in stochastic games. In Bernhard Nebel, editor, Proceedings of the 17th International Joint Conference on Artificial Intelligence (IJCAI’01), pages 1021–1026, Seattle, Washington, August 4 - 10 2001. Morgan Kaufmann.

[6] Wilfried Brauer and Gerhard Weiß. Multi-machine scheduling - a multiagent learning approach. In Proceedings of the 3rd International Conference on Multi-Agent Systems (ICMAS’98), pages 42–48, Paris, France, July 4 -7 1998. IEEE Press.

[7] Peter Brucker. Scheduling Algorithms. Springer Verlag, Berlin, Germany, second edition, 1998.

[8] Ivan D. Chase, Marc Weissburg, and Theodore H. Dewitt. The vacancy chain process: a new mechanism of resource distribution in animals with application to hermit crabs. Animal Behavior, 36:1265–1274, 1988.

[9] Daniel D. Corkill and Victor R. Lesser. The use of meta-level control for coordination in a distributed problem solving network. In Proceedings of the 8th International Joint Conference on Artificial Intelligence (IJCAI’83), volume 2, pages 748–756, Karlsruhe, West Germany, August 8 - 12 1983. William Kaufmann.

[10] Torbjørn S. Dahl, Maja J. Matarić, and Gaurav S. Sukhatme. Adaptive spatio-temporal organization in groups of robots. In Proceedings of the 2002 IEEE/RSJ International Conference on Intelligent Robots and Systems (IROS’02), pages 1044–1049, Lausanne, Switzerland, September 30 - October 4 2002. IEEE Press.

[11] Brian P. Gerkey and Maja J Matarić. Sold!: Auction methods for multirobot coordination. IEEE Transactions on Robotics and Automation, 18(5):758–768, October 2002.

[12] Brian P. Gerkey and Maja J. Matarić. A formal framework for the study of task allocation in multi-robot systems. Technical Report CRES-03-013, University of Southern California, Center for Robotics and Embedded Systems, 2003.

[13] Brian P. Gerkey and Maja J Matarić. A framework for studying multi-robot task allocation. In A. C. Schultz et al., editors, Multi-Robot Systems: From Swarms to Intelligent Automata, Volume II, Proceedings of the 2nd International Naval Research Laboratory Workshop on Multi-Robot Systems, Washington, DC, March 17 - 19 2003.

[14] Brian P. Gerkey, Richard T. Vaughan, Kasper Støy, Andrew Howard, Gaurav S. Sukhatme, and Maja J Matarić. Most valuable player: A robot device server for distributed control. In Proceedings of the 2001 IEEE/RSJ International Conference on Intelligent Robots and Systems (IROS’01), pages 1226–1231, Wailea, Hawaii, October 29 - November 3 2001. IEEE Press.

[15] Dani Goldberg and Maja J Matarić. Learning multiple models for reward maximization. In Pat Langley, editor, Proceedings of the 17th International Conference on Machine Learning (ICML’00), pages 319–326, Stanford, California, June 29 - July 2 2000. Morgan Kaufmann.

[16] Dani Goldberg and Maja J Matarić. Design and evaluation of robust behavior-based controllers for distributed multi-robot collection tasks. In Tucker R. Balch and Lynne E. Parker, editors, Robot Teams: From Diversity to Polymorphism, pages 315–244. A K Peters Ltd, 2001.

[17] Kwun Han and Manuela M. Veloso. Automated robot behavior recognition applied to robotic soccer. In Proceedings of the 9th International Symposium on Robotics Research (ISRR’99), pages 199–204, Snowbird, Utah, October 9 - 12 1999.

[18] Owen Holland and Chris Melhuish. Stigmergy, self-organization and sorting in collective robotics. Artificial Life, 5(2):173–202, 1999.

[19] Boyoon Jung and Gaurav S. Sukhatme. Tracking targets using multiple robots: The effect of environment occlusion. Autonomous Robots, 13(3):191–205, 2002.

[20] Kristina Lerman, Asram. Galstyan, Alcherio Martinoli, and Auke J.

Ijspeert. A macroscopic analytical model of collaboration in distributed robotic systems. Artificial Life, 7(4):375–393, 2001.

[21] Michael L. Littman. Markov games as a framework for multi-agent reinforcement learning. In William W. Cohen and Haym Hirsh, editors, Proceedings of the 11th International Conference on Machine Learning (ICML’94), pages 157–193, New Brunswick, New Jersey, July 10 - 13 1994. Morgan Kaufmann.

[22] Maja J. Matarić. Interaction and Intelligent Behavior. PhD thesis, Massachusetts Institute of Technology, Cambridge, Massachusetts, 1994.

[23] Maja J. Matarić, Gaurav S. Sukhatme, and Esben Østergaard. Multirobot task allocation in uncertain environments. Autonomous Robots, 14(2- 3):255–263, 2003.

[24] Roger B. Myerson. Game Theory: Analysis of Conflict. Harvard University Press, Cambridge, Massachusetts, 1991.

[25] Esben Østergaard, Gaurav S. Sukhatme, and Maja J. Matarić. Emergent Bucket Brigading - A simple mechanism for improving performance in multi-robot constrained-space foraging tasks. In Proceedings of the 5th International Conference on Autonomous Agents (Agents’01), pages 29–30, Montreal, Canada, May 28 - June 1 2001. ACM Press.

[26] Lynne E. Parker. L-ALLIANCE: Task-Oriented Multi-Robot Learning in Behaviour-Based Systems. Advanced Robotics, Special Issue on Selected Papers from IROS’96, 11(4):305–322, 1997.

[27] Anil K. Seth. Modelling group foraging: Individual suboptimality, interference, and a kind of matching. Adaptive Behavior, 9(2):67–91, 2001.

[28] Richard S. Sutton and Andrew G. Barto. Reinforcement learning: an introduction. MIT Press, Cambridge, Massachusetts, 1998.

[29] Poj Tangamchit, John M. Dolan, and Pradeep K. Khosla. Learning-based task allocation in decentralized multirobot systems. In Lynne E. Parker, George Bekey, and Jacob Barhen, editors, Distributed Autonomous Robotic Systems 4, Proceedings of the 5th International Symposium in Distributed Autonomous Robotic Systems (DARS’00), pages 381–390, Knoxville, Tennessee, October 4 - 6 2000. Springer.

[30] Barry B. Werger and Maja J Matarić. Broadcast of local eligibility for multi-target observation. In Lynne E. Parker, George Bekey, and Jacob Barhen, editors, Distributed Autonomous Robotic Systems 4, Proceedings of the 5th International Symposium on Distributed, Autonomous Robotic Systems (DARS’00), pages 347–356, Knoxville, Tennessee, October 4-6 2000. Springer.

[31] Helen Yan and Maja J Matarić. General spatial features for analysis of multi-robot and human activities from raw position data. In Proceedings of the 2002 IEEE/RSJ International Conference on Intelligent Robots and Systems (IROS’02), pages 2770–2775, Lausanne, Switzerland, September 30 - October 4 2002. IEEE Press.

[32] Wei Zhang and Thomas G. Dietterich. A reinforcement learning approach to job-shop scheduling. In Proceedings of the 14th International Joint Conference on Artificial Intelligence (IJCAI’95), pages 1114–1120, Montréal, Canada, August 20 - 25 1995. Morgan Kaufmann.

[33] Albert Y. Zomaya, Mathew Clements, and Stephan Olariu. A framework for reinforcement-based scheduling in parallel processor systems. IEEE Transactions On Parallel and Distributed Systems, 9(3):249–259, March 1998.